ILL 066

**Network Level Activation Capability**

**Origination Date :**11/08/1996

**Originator:**Ameritech

**Description:**

The NPAC SMS should provide the capability to process activate messages down to the network element level.  This would require the NPAC-LSMS interface to support asynchronous responses from the LSMS for activation responses to the SCP level.

**Final Resolution:**

This feature has been requested for Release 4.  Detailed requirements need to be developed.

Withdrawn by originator.

**Related Release:**

N/A

**Status:** Closed