ILL 187

**NXX split handling for 6 digit**

**Origination Date :**02/22/1997

**Originator:**AT&T;

**Description:**

Currently there are no requirements or functionality in the NPAC SMS to address NPA-NXX splits, only NPA splits.  This is needed for an NPA-NXX where the split requires TNs to be changed to a new NPA and a new NXX.  Further investigation and requirements development needs to be done to support this functionality.

**Final Resolution:**

Backwards Compatible:  NO

This feature has been requested for a future release.  Detailed requirements need to be developed. This change has not been associated with a group.

Change order withdrawn by the originator.

This change order has been reopened and placed on hold due to issues raised in the Western Region.

Oct LNPAWG (KC), group votes to move to cancel-pending.

**Related Release:**

N/A

**Status:** Closed