NANC 078

**OID usage and NpacAssociationUserInfo**

**Origination Date:** 04/22/1997

**Originator:** Lockheed Martin

**Description:**

NpacAssociationUserInfo should be made a lnpAttribute so that it has an OID that can be used in the UserInfo field. Currently we are using the ASN.1 OID.   
   
Listed below are the OID’s being used.  These should be documented in the IIS.  
   
OIDs Used for BIND REQUESTS:  
·     CMIPUserInfo OID = 2:9:1:1:4  
    (per standards and pp49 IIS1.5)  
·     CMIPAbortInfo OID = 2:9:1:1:4  
    (per standards and  pp51 IIS1.5)  
·     LnpAccessControl OID = {lnp-attribute 1} =  
1:3:6:1:4:1:103:7:0:0:2:1  
·     UserInfo (NpacAssociationInfo) OID =  
1:3:6:1:4:1:103:7:0:0:2:105  
·     Application context = OID 2:9:0:0:2  
    (per standards)  
   
OTHER OIDs of INTEREST:  
·     AccessControl OID as part of a SMI notification = 1:3:6:1:4:1:103:7:0:0:8:1  
accessControl as part of LNP notifications ={lnp-attribute 1} =  1:3:6:1:4:1:103:7:0:0:2:1

**Final Resolution:**

Add an attribute definition for NpacAssociationUserInfo to be standards compliant. The OIDs would be documented in the IIS.

New ASN.1 and GDMO are available on the web as of 5/2.  The IIS will be updated in the 1.1.

**Related Release:**

1.1

**Status:** Implemented