NANC 103B

**Increase in OSI Selector Size**

**Origination Date:** 05/23/1997

**Originator:** AT&T

**Description:**

Currently in the IIS and FRS the OSI TSAP, SSAP, and PSAP sizes are limited to 4 characters.  It has been requested that these be increased in size.

**Final Resolution:**

Func Backwards Compatible:  NO

The selector would be defined as a range from 4…16 or 20.

June 00 LNPAWG meeting, group consensus (during R5 discussion) is to move to cancel-pending.

Sept 00 LNPA WG meeting – move to deleted.

**Related Release:**

N/A

**Status:** Closed