NANC 106

**Digital Signature Definitions**

**Origination Date:** 06/07/1997

**Originator:** AGCS

**Description:**

The IIS NANC1.1, paragraph 5.2.1.10 Signature, states that the fields specified in the LnpAccessControl are converted to either ASCII or Integer types, and then hashed/encrypted.  Some of these conversions are obvious.  However, it has been requested that the following information be included in the IIS.

|  |  |  |
| --- | --- | --- |
|  **Field**  |  **Format**  |  **Comments**  |
|  systemId  |  ASCII  |  |
|  systemType  |  Integer  |  e.g. local-sms = 1  |
|  userId  |  ASCII  |  |
|  cmipDepartureTime  |  ASCII  |  format of “YYYYMMDDHHMMSS.0Z  |
|  sequenceNumber  |  Integer  |  |

**Final Resolution:**

This information will be added in IIS 1.3 and IIS 2.1.

**Related Release:**

1.3

**Status:** Implemented