NANC 106

**Digital Signature Definitions**

**Origination Date:** 06/07/1997

**Originator:** AGCS

**Description:**

The IIS NANC1.1, paragraph 5.2.1.10 Signature, states that the fields specified in the LnpAccessControl are converted to either ASCII or Integer types, and then hashed/encrypted.  Some of these conversions are obvious.  However, it has been requested that the following information be included in the IIS.

|  |  |  |
| --- | --- | --- |
| **Field** | **Format** | **Comments** |
| systemId | ASCII |  |
| systemType | Integer | e.g. local-sms = 1 |
| userId | ASCII |  |
| cmipDepartureTime | ASCII | format of    “YYYYMMDDHH MMSS.0Z |
| sequenceNumber | Integer |  |

**Final Resolution:**

This information will be added in IIS 1.3 and IIS 2.1.

**Related Release:**

1.3

**Status:** Implemented