NANC 141

**Cancel of Disconnect Pending**

**Origination Date :**08/18/1997

**Originator:**Lockheed Martin Team

**Description:**

The requirement R5-71.10 states “NPAC SMS shall set the subscription version status to Active upon receiving a cancellation for a subscription version with a status of disconnect pending.”.  However, there are requirements R5-3.10, R5-3.11, and R5-3.12 that define a tunable parameter for retention of canceled versions with a pre-cancellation status of disconnect pending.  This tunable is not needed and should be removed.  The requirements R5-3.10, R5-3.11, R5-3.12 and the reference to the tunable in the table in appendix C should be removed.

**Final Resolution:**

The FRS should be updated in the next release.

Closed for FRS release 1.5.

**Related Release:**

1.5

**Status:** Implemented