NANC 151

**TN and Number Pool Block Addition to Notifications**

**Origination Date :**09/04/1997

**Originator:**Bellcore

**Description:**

It has been requested that the TN for the subscription version be added to all notifications that currently contain SV-ID but not TN from the NPAC SMS.  It is possible for a SOA in a disconnect or modify-active situation, to not have the SV record in their database.  Therefore, when the attribute/status change notification comes from the NPAC SMS, there is no way to correlate its version id with the TN on the disconnect or modify request in SOA.

Jun 00 LNPA-WG meeting, additionally, the same type of change should be done for Number Pool Block (i.e., add the NPA-NXX-X to all notifications that currently contain Block-ID but not NPA-NXX-X).

**Final Resolution:**

Func Backwards Compatible:  NO

**This would be a deviation from the standard since the TN would not have been an attribute that has changed.**

This is an "OLD" Release 2.0 change order, that has been moved into the "Accepted" category, awaiting prioritization

Implemented in FRS 3.3.0a, GDMO 3.3.0 and ASN.1 3.3.0.

**Related Release:**

Implemented in FRS 3.3.0a, GDMO 3.3.0 and ASN.1 3.3.0.

**Status:** Implemented