NANC 155

**End User Location Type and Value Definition**

**Origination Date :**08/05/1997

**Originator:**AT&T;

**Description:**

In the NANC IIS V1.2 the following ASN.1 definitions are found:

EndUserLocationType ::= CHOICE {

  value [0] NumberString(SIZE2)),

  no-value-needed [1] NULL

}

EndUserLocationValue ::= CHOICE {

  value [0] NumberString(SIZE(1..12)),

  no-value-needed [1] NULL

}

However, in the FRS V1.2 the following is found in Table 3-5:

End User Location Type C(2)

End User Location Value C(12)

where "C" is defined as "Character or Alphanumeric Strings".

**Final Resolution:**

At, at this time since these fields are not being used this change order will sync the FRS with the IIS.  The values in the table will be changed to N(2) and N(12) from C(2) to C(12).  In the long term these fields will be fixed in change order NANC 129.

This change order has been added to the NANC 1.6 documents**.**

**Related Release:**

1.6

**Status:** Implemented