NANC 189

**Service Provider Allowable Functions Modification**

**Origination Date :**01/19/1998

**Originator:**ESI

**Description:**

NPAC FRS requirement R4-15.1 - where it states - NPAC SMS shall allow Service Provider data to be modified or added to the Service Provider data with the exception of the data listed in table 3-2.The Allowable Functions is part of table 3-2.  However, in the GDMO for the IIS the allowable functions are defined as GET-REPLACE.

Functionality needs to be verified by both NPAC vendors to determine the actual functionality that was implemented and the action that needs to be taken.

**Final Resolution:**

Backwards Compatible:  YES

Lockheed and Perot to verify their implementations.  Specifically vendors must determine if they allow allowable functions to be changed over the CMIP interface and what the behavior would be if the data were changed.  For example, would the association be aborted or would the change take effect for future associations?

Lockheed does not support the changing of the data over the CMIP interface.  Perot does support this functionality.  The group determined that the FRS takes precedence. This functionality is not anticipated to be needed in the future for live operations. The IIS GDMO should be changed to GET from GET-REPLACE for this attribute.

This change order is a low priority.

Sep LNPA-WG (Chicago), the group agreed to make this a doc-only change order.  The GDMO change from GET-REPLACE to GET should be done.

**Related Release:**

3.0.1

**Status:** Implemented