**NANC 256**

**First Port Notifier for New NPA-NXX in an NPA Split**

**Origination Date :**01/12/1999

**Originator:**ESI

**Description:**

Jim Rooks requested that we discuss/document the behavior for the current functionality of the first port notifier.  Currently, the NPAC sends out a first port notification of an SV Create for a New NPA-NXX involved in a split, regardless of SVs that may have been moved from the Old NPA-NXX at the start of PDP.

This new requirement will go in the same FRS section as RR5-3, which defines first port notifiers (the underlined words define the differences between the existing requirement and the proposed new requirement).

*Req 1 – Create Subscription Version – Notify NPA-NXX First Usage of a New NPA-NXX involved in an NPA Split*

*NPAC SMS shall notify all accepting Local SMSs and SOAs of the NPA-NXX, effective date, and owning Service Provider when a New NPA-NXX involved in an NPA Split, is being ported for the first time, after the start of Permissive Dialing, immediately after creation validation of a Subscription Version.*

**Final Resolution:**

Jan LNPAWG (Atlanta), John will write up description for next meeting.

Feb LNPAWG (San Ramon), group O.K. with this change order.  Move to next doc category.

**Related Release:**

2.0.1

**Status:** Implemented