**NANC 262**

**FRS Documentation Change**

**Origination Date :**02/03/1999

**Originator:**CMA

**Description:**

Re-send of activation request (RR5-38.4) should have reference to modification removed, and a new requirement (in the re-send section, RR5-38.9) should be added to reflect the re-send of an active SV that failed the initial modify active request.  Also, update RR5-38.5 to have consistent words.

**RR5-38.4  Resend Subscription Version - Activation Request**

NPAC SMS shall resend a Subscription Version activation request, if ~~either~~ the Subscription Version previously failed activation ~~or an active Subscription Version previously failed modification~~ , to the designated list of failed Local SMSs via the NPAC SMS to Local SMS Interface upon a Subscription Version resend request.

**RR5-38.9  Resend Subscription Version – Modification Request**

NPAC SMS shall resend a Subscription Version modification request, if an active Subscription Version previously failed modification, to the designated list of failed Local SMSs via the NPAC SMS to Local SMS Interface upon a Subscription Version resend request.

**RR5-38.5  Resend Subscription Version – Disconnect Request**

NPAC SMS shall resend a Subscription Version disconnect request, if the Subscription Version **previously** failed disconnect, to the designated list of failed Local SMSs **via the NPAC SMS to Local SMS Interface** upon a Subscription Version resend request.

**Final Resolution:**

Feb LNPAWG (San Ramon), group O.K. with this change order.  Move to next doc category.

**Related Release:**

2.0.1

**Status:** Implemented