**NANC 270**

**Documentation change for Re-Send**

**Origination Date :**03/16/1999

**Originator:**National Number Pooling Sub-Com'ttee

**Description:**

While reviewing the Natl N Pool test cases, it was noted that the re-send functionality is not documented in the FRS.  It has been requested by the subcommittee to update this information in the FRS.

Section 5.1.2.2.7 Subscription Version Resend

Existing Requirement (text stays the same, new number is RR5-38.1.1):

RR5-38.1   Resend Subscription Version - Identify Subscription Version

NPAC SMS shall receive the following data from NPAC personnel to identify a ~~failed or partial failure~~ subscription version that contains a Failed SP List with one or more SPIDS, to be resent:

Ported Telephone Number

Or

Subscription Version ID

New Requirement:

RR5-38.1.2  Resend Subscription Version - Identify Multiple Subscription Versions

NPAC SMS shall require NPAC personnel to specify a TN Range (NPA-NXX-xxxx through yyyy, where yyyy is greater than xxxx) to identify multiple ~~failed or partial failure~~ subscription versions that contain a Failed SP List with one or more SPIDS, to be resent.

**Final Resolution:**

Backwards Compatible:  YES

Apr LNPAWG (DC), remove time range and NPA-NXX range.

This will be put into the queue of CMA updates to the FRS.  No date has been scheduled.

**Related Release:**

3.0.0

**Status:** Implemented