**NANC 278**

**FRS Documentation - SV requirements**

**Origination Date :**04/05/1999

**Originator:**AT&T;

**Description:**

Several requirements need to be updated in the 2.0.0 FRS.  Deleted words are struck-through, and new words are highlighted.

R5‑66.2   Disconnect Subscription Version Complete - Set Disconnect Broadcast Complete Date

NPAC SMS shall *update* ~~set~~ the Disconnect Broadcast Complete timestamp *of* ~~to the current date in~~ the previously active~~, now old,~~ Subscription Version upon *completion of the broadcast, and the FIRST* ~~a~~ successful *response* ~~disconnect~~ from *a* ~~one~~ Local SMS.

R5‑66.3   Disconnect Subscription Version Complete - Set Disconnect to Old

NPAC SMS shall set the ~~sending~~ disconnect Subscription Version to old *if* ~~upon~~ a successful *response from at least one* ~~disconnect in all~~ Local SMSs *is returned* .

R5‑66.4   Disconnect Subscription Version Complete – Status Update of SV (new requirement)

*NPAC SMS shall update the status of the disconnect Subscription Version upon completion of the Deletion broadcast, and a response from ALL Local SMSs, or retries are exhausted.*

R5-40.5    Modify Active Subscription Version – Modify Broadcast Complete Time Stamp Update (new requirement)

*NPAC SMS shall update the Modify Broadcast Complete Timestamp of a Subscription Version upon completion of the broadcast, and the FIRST successful response, from a Local SMS.*

R5-40.6    Modify Active Subscription Version – Status Update of SV (new requirement)

*NPAC SMS shall update the status of the modify active Subscription Version upon completion of the Modify Broadcast, and a response from ALL Local SMSs, or retries are exhausted.*

**Final Resolution:**

Apr LNPAWG (DC), group O.K. with this change order.  Move to next doc list.

**Related Release:**

2.0.1

**Status:** Implemented