**NANC 289**

**R3 Requirements Update – documentation only – from Pooling Assumptions walk-thru**

**Origination Date :**05/27/1999

**Originator:**TSE

**Description:**

During the Pooling Assumptions call on 5/26, several requirement updates were discussed.  Numbers were assigned to be the appropriate requirement numbers according to where the new requirements should be inserted in the documentation.

Remove SV-428.1 - 428.7.

Remove "partial failure/failed" from SV230, SV240, SV270, and SV280.  (to be added to existing change order 227)

Add N-270

The NPAC SMS shall reject a request to delete (de-pool) an NPA-NXX-X if there is an SV with a status of sending as a result of a disconnect request.

Add SV-429

Once an NPA-NXX-X-Deletion has begun, the NPAC SMS shall ensure at completion that no SVs exist with LNP Type of POOL.

In addition, the Pooling Assumption call on 5/19 made the following updates:

Added text <> to N-365

NPAC SMS shall provide to NPAC Personnel only, an indicator on the NPAC Administrative Interface <only after a query> if an associated Block Create Scheduled Event, that has not been executed, exists in the NPAC SMS.

**Final Resolution:**

Backwards Compatible:  YES

Jul LNPAWG (Ottawa), move to next doc category.

Aug LNPAWG (Portland), need to remove B-169.1.3 since the error message references SV-428.x, and all of these requirements have been removed.

**Related Release:**

3.0.0

**Status:** Implemented