NANC 434

**VoIP SP Type**

**Origination Date :**03/12/2008

**Originator:**LNPA-WG

**Description:**

**Business Need:**

During the discussion of FCC Order 07-188, participants agreed that the SP Type values should be modified to align with the definition in the Order.

 VoIP SP Type in the FRS-- In the data model section (NPAC Customer data model – table 3-2), the text for “SP Type3” should be replaced with “class1Interconnected VoIP”.

**Final Resolution:**

Backward Compatible:  YES

Update the FRS accordingly.

Implemented in FRS 3.4.0a 3/19/10

 Implemented in 3.4.0 ASN.1/GDMO

**Related Release:**

Implemented in FRS 3.4.0a 3/19/10

 Implemented in 3.4.0 ASN.1/GDMO

**Status:** Implemented