**Origination Date:** 8/18/09

**Originator:** NeuStar

**Change Order Number: NANC 439 Description:** Doc-Only Change Order: FRS Updates

**Cumulative SP Priority, Average:** not rated, included **Functional Backward Compatible:** YES **IMPACT/CHANGE ASSESSMENT**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| FRS | IIS | GDMO | ASN.1 | **NPAC** | SOA | LSMS |
| Y | N | N | N | None | None | None |

**Business Need:**

Per approval by the NAPM LLC (SOW 75 for “Elimination of Dial-Up Port to NPAC Network”), there is the elimination of all existing dial-up access arrangements for NPAC LTI users. As such, the text in the FRS needs to remove all references to dial-up access.

**Description of Change:** Update the FRS. **Requirements:**

R7-41 System Access, User Authentication Procedure Entry – ~~Dial-Up~~SSL VPN Limitations

NPAC SMS shall provide a mechanism to limit the users authorized to access the system via ~~dial-up~~SSL VPN facilities.

R7-43.3 ~~Dial-Up~~SSL VPN Access

NPAC SMS shall use smart cards to authenticate users accessing the NPAC SMS via ~~dial-up~~SSL VPN.

IIS:

No change required. GDMO:

No change required. ASN.1:

No change required.