NANC 062

**Filter NPA-NXX Object Behavior Description/Modification**

**Origination Date:** 04/03/1997

**Originator:** Lockheed Martin

**Description:**

The description for the LSMS filter object is inconsistent in the IIS.  Exhibit 6 shows the object is available for modification from the SOA.  There are flows for the SOA in the NANC 1.0 release.  However, exhibit 7 and the lnpFilterNPA-NXX object behavior conflict with the sections mentioned above and are inconsistent with the requirements.

The direction (to/from) column for the filter Exhibit 7 should be updated for LSMS Filter NPA-NXX Create/Delete/Query to show from SOA in addition to from LSMS.

The GDMO should be modified to state the following:

NPAC SMS Managed Object used for the Local SMS to NPAC SMS interface and the NPAC SMS to SOA interface.

All attributes are read only.  Once, created the lsmsFilterNPA-NXX object can be deleted via the Local SMS or SOA.  The lsmsFilterNPA-NXX-ID is specified by the NPAC SMS.

The Local SMS or SOA can M-DELETE, M-CREATE, and M-GET the lsmsFilterNPA-NXX objects on the NPAC SMS. (Network Data Association Function).

**Final Resolution:**

IIS modifications will be made in the 1.1 release.

**Related Release:**

1.1

**Status:** Implemented