NANC 098

**TSAP data required in FRS**

**Origination Date:** 05/22/1997

**Originator:** Lockheed Martin

**Description:**

Table 3-4 in the FRS, NPAC Customer Network Address Data Model, indicates that the TSAP is not a required field, unlike the other selectors.  The table should be changed to make the TSAP field required.

**Final Resolution:**

The FRS updates would be made in release 1.2.

**Related Release:**

1.2

**Status:** Implemented