# NANC 103A

## Clock Synchronization 5 or 2 Minutes

**Origination Date:** 05/31/1997

**Originator:** Lockheed Martin Team

### Description:

In Chapter 5 of IIS section 5.2.1.6 states clock synchronization should be within 2 minutes, but in another section it states 5 minutes.

Per the following requirement it should be 5 minutes:  
   
R7-105.2 Generalized Time  
SOA to NPAC SMS interface and the NPAC SMS to Local SMS interface shall ensure that external messages received have a generalized time in the access control information within 5 minutes of the NPAC SMS system clock.

**Final Resolution:**

IIS 1.3 and or 2.1 will be updated.

**Related Release:**

1.3

**Status:** Implemented