NANC 118

**CMIP Notification Recovery by Time Range**

**Origination Date :**06/27/1997

**Originator:**Lockheed Martin

**Description:**

It has been requested that CMIP notification recovery be requested by time range as, as done in LSMS download actions.  The IIS action definition contains time range per NANC 113.

The text is currently as follows:

RR6-14 CMIP Notification Recoverability

The non-recoverable CMIP notifications should be recoverable over the NPAC SMS to Local SMS and SOA to NPAC SMS interfaces. ….

The text should be changed as follows:

RR6-14 CMIP Notification Recoverability

The non-recoverable CMIP notifications should be recoverable using time range over the NPAC SMS to Local SMS and SOA to NPAC SMS interfaces.….

**Final Resolution:**

This change would be documented in FRS 2.X

This change order has been merged with ILL 79.

**Related Release:**

2.0.0

**Status:** Implemented