NANC 137

**Disconnect Active SV Behavior Clarification**

**Origination Date :**08/13/1997

**Originator:**Lockheed Martin

**Description:**

We have a conflict between the FRS and the GDMO dealing with disconnecting active subscription versions. In the FRS, requirement R5-64.1 states that we shall not allow a disconnect of an active SV if there is a "pending" SV for that same TN until that "pending" SV is cancelled.

In the GDMO in IIS 1.2, section 5.0, Action Behaviors, states  “there is a pending SV and an active SV, and the currentSP has not authorized the port, the active one will be disconnected, and the pending one will go into conflict. If the SP has not  authorized the port, the disconnect will fail”

The GDMO should be corrected to state, “if there is a pending SV and an active SV, the disconnect of the active SV will fail.”

**Final Resolution:**

IIS would be updated in the next release.

Pending review.

Move to closed.

**Related Release:**

1.5

**Status:** Implemented