NANC 162

**TN-Attribute as GET-Replace**

**Origination Date :**09/26/1997

**Originator:**AGCS

**Description:**

The TN attribute in the SV should be read only.  Due to historical reasons the attribute was get replace due to different implementation discussed for NPA splits.

**Final Resolution:**

The group has accepted this ANS.1 modification.  It is a recompile change only.

This is in Release 2 (SOW 9).

**Related Release:**

2.0.0

**Status:** Implemented