NANC 178

**NANC 048 Clarifications**

**Origination Date :**11/25/1997

**Originator:**ESI

**Description:**

The following changes have been requested for clarification in NANC 48:

Requirement 7 - Association Rejection for Associated Service Provider Id

NPAC SMS shall reject any SOA to NPAC SMS association attempt by a Service Provider Id that is a service provider associated with the primary Service Provider Id in the NPAC Customer Associated Service Provider Information.

Wording change made above to make it clearer that the associated service provider association is rejected.  This requirement would then be in sync with Assumption 1.

Constraint 1 - Associated Service Provider Notification Aggregation

NPAC SMS aggregation of notifications for primary and associated service provider ids will not be supported by the NPAC SMS.

Should be modified to state ...aggregation of all messages over the SOA to NPAC SMS interface….."

Requirements 12 - Filters for Associated Service Providers

NPAC SMS shall apply filters for the associated Service Provider Id before sending them over the SOA to NPAC SMS interface association for the primary service provider.

Should be changed to state "...apply NPA and/or NPA-NXX (accepted) filters...."

**Final Resolution:**

The group has accepted this change.  Submission to the LLC’s has occurred.

This is in Release 2 (SOW 9).

**Related Release:**

2.0.0

**Status:** Implemented