NANC 200

**Notification of NPA Splits**

**Origination Date :**02/28/1998

**Originator:**AGCS

**Description:**

It has been requested that to facilitate synchronization during NPA split, the NPAC via the mechanized interface should notify the SOA and LSMSs. The preferred method would be to have a new managed object that contains all split information. It would still be up to the respective system to perform the splits, but all systems would be in sync. A second alternative would be to have the NPAC issue a notification that states the NPAC is start/ending split processing.

**Final Resolution:**

Func Backwards Compatible:  NO

This change order is related to change order NANC 192 that proposes getting the split information from the LERG.

**01/02/02** – NPAC R4.0 as submitted to the LLC in 2000 is not going forward.  This change order has been moved back into the “accepted” section of this document.

**12/05**– Moved to Cancel-Pending per LNPAWG discussion.

3/06 – moved to Deleted after March LNPAWG meeting

**Related Release:**

N/A

**Status:** Closed