NANC 210

**IIS Flow 6.5.1.12 Modification**

**Origination Date :**12/31/1969

**Originator:**

**Description:**

IIS Flow 6.5.1.12 "Subscription Version Port to Original: Success", states in b., e., and g. that the status is set to "Sending" when an activate is received for a Port to Original, and that status sent to the old and new SP. The NPAC actually sends a status of "Disconnect-Pending".  This status only lasts for a few seconds but does result in a notification to the old and new SP.  This has not been an issue for any of the SPs during certification but is an inconsistency between the IIS and the NPAC.

**Final Resolution:**

Submitter is reviewing this change order for accuracy.  This change order may be withdrawn.

Closed no action by submitter 4/14/1998.

**Related Release:**

N/A

**Status:** Closed