**NANC 242**

**Documentation Change to FRS for R7-96**

**Origination Date :**10/20/1998

**Originator:**TSE

**Description:**

The FRS incorrectly lists the elements of the digital signature.  It states:  unique id of sender, generalized time of msg issuance, sequence number, key id, key list.

The list should be as stated in the IIS:  system ID, system type, user ID, departure time, sequence number.

**Final Resolution:**

The documentation should be updated in the next version of the FRS.

**Related Release:**

2.0.1

**Status:** Implemented