**NANC 255**

**GDMO Documentation Changes**

**Origination Date :**01/07/1999

**Originator:**ESI

**Description:**

The following changes were discovered during the R2 review.

1. In all the behavior for DPC attributes:  
   The data is stored in BCD (e.g., a value of FFF would be displayed as 255.255.255).  
     
   Change FFF to FFFFFF

      2.  Under the lnpDownload Action definition, it should state (new words in *larger print italics* ):  The lnpDownload action is the action that is used by the Local SMS *and      SOA* to specify the objects to be downloaded from the NPAC SMS.

**Final Resolution:**

Jan LNPAWG (Atlanta), John will write up description.

Group O.K. with this change order.  Move to next documentation list.

**Related Release:**

2.0.1

**Status:** Implemented