**NANC 266**

**ASN.1 Change**

**Origination Date :**02/25/1999

**Originator:**AGCS

**Description:**

A change to the Release 2.0 ASN.1 has been discovered.  Specifically, the “tagging” for a sequence needs to be changed, based on the 1.6 ASN.1.

1.6

VersionCreateConcurrenceRequest ::= SEQUENCE {

   tn PhoneNumber,

   version-id LnpKey,

   service-prov-id ServiceProvId,

   service-prov-due-date GeneralizedTime,

   service-prov-authorization-creation-time-stamp

         GeneralizedTime,

   access-control LnpAccessControl

}

v2.0.0

VersionCreateConcurrenceRequest ::= SEQUENCE {

   tn [0] PhoneNumber,

   version-id [1] LnpKey,

   service-prov-id [2] ServiceProvId,

   service-prov-due-date [3] GeneralizedTime,

   service-prov-authorization-creation-time-stamp [4]

         GeneralizedTime,

   access-control [5] LnpAccessControl,

   subscription-timer-type [6] Integer OPTIONAL,

   subscription-business-type [7] Integer OPTIONAL

}

The fix would be to only tag the last 2 new fields:

   Subscription-timer-type [0] Integer OPTIONAL,

   subscription-business-type [1] Integer OPTIONAL

**Final Resolution:**

The final ASN.1 is shown below:

VersionCreateConcurrenceRequest ::= SEQUENCE {

   tn PhoneNumber,

   version-id LnpKey,

   service-prov-id ServiceProvId,

   service-prov-due-date GeneralizedTime,

   service-prov-authorization-creation-

          timestamp GeneralizedTime,

   access-control LnpAccessControl,

   subscription-timer-type [0] Integer

         OPTIONAL,

   subscription-business-type [1] Integer

         OPTIONAL

}

**Related Release:**

2.0.1

**Status:** Implemented