NANC 338

**Doc Only Change Order for FRS: Add requirement for NPAC SMS sending subscriptionVersionDonorSP-CustomerDisconnectDate notifications to the Donor SP SOA when a Number Pool Block De-Pool occurs and update the note in requirement RR5-85.**

**Origination Date :**10/05/2001

**Originator:**R3.1 Test Review Group

**Description:**

RR5-85 Currently reads:

**RR5-85 Number Pooling Subscription Version Information – Suppression of Notifications**

NPAC SMS shall suppress status change and attribute value change notifications to the old and new/current service provider SOA systems for Subscription Versions with LNP Type of POOL.  (Previously SV-2)

NOTE:  This includes creation, modification, deletion, re-send, resync, audits, and mass update.  An exception to the deletion is the donor disconnect notification in a de-pool situation.  This notification will still be sent to the Code Holder, which informs the Code Holder of the responsibility to provide vacant number treatment upon a de-pool of a 1K Block.  This notification is the same that is sent for a disconnect of a ported SV in a non-pooling environment.

RR5-85 is amended to read:

**RR5-85 Number Pooling Subscription Version Information – Suppression of Notifications**

NPAC SMS shall suppress status change and attribute value change notifications to the old and new/current service provider SOA systems for Subscription Versions with LNP Type of POOL.  (Previously SV-2)

NOTE:  This includes creation, modification, deletion, re-send, resync, audits, and mass update. ~~An exception to the deletion is the donor disconnect notification in a de-pool situation.  This notification will still be sent to the Code Holder, which informs the Code Holder of the responsibility to provide vacant number treatment upon a de-pool of a 1K Block.  This notification is the same that is sent for a disconnect of a ported SV in a non-pooling environment.~~

Requirement to be added:

**RR5-85.5 Number Pooling Subscription Version Information – Disconnect Notifications to Donor Service Provider**

NPAC SMS shall send donor disconnect notifications to the Donor Service Provider (Code Holder) when a Number Pool Block De-pool occurs.

**Final Resolution:**

Corresponding IIS Doc Only Change Order is NANC 339

Incorporate into next release of FRS.

**11/14/01** – Reviewed at November 2001 LNPA WG.  NeuStar has verified that the implementation supports the new requirement.

Service Providers to verify internally that this change order does not have an impact on their local systems. Leave in “open” status until December 2001 meeting.

**12/12/01** – Move to ‘accepted’.

**Related Release:**

Implemented in FRS 3.2.0.

**Status:** Implemented