NANC 339

**Doc Only Change Order for IIS: Flow B.4.4.24 to include the Donor Disconnect notifications that get sent to the Donor SOA when a Number Pool Block De-pool occurs.**

**Origination Date :**10/05/2001

**Originator:**R3.1 Test Review Group

**Description:**

Steps will be inserted in the flow diagram and the flow text between the existing steps 8 and 9 as follows:

NPAC SMS sends, depending upon the donor service provider’s TN Range Notification Indicator, a subscriptionVersionDonorSP-CustomerDisconnectDate or subscriptionVersionRangeDonorSP-CustomerDisconnectDate notification to the donor service provider SOA that the subscription version is being disconnect with the customer disconnect date.

The donor service provider SOA confirms the M-EVENT-REPORT.

**Final Resolution:**

Corresponding FRS Doc Only Change Order is NANC 338.

 Incorporate into next release of IIS.

**11/14/01** – Reviewed at November 2001 LNPA WG.  NeuStar has verified that the implementation supports the new requirement.  Service Providers to verify internally that this change order does not have an impact on their local systems. Leave in “open” status until December 2001 meeting.

**12/12/01** – Move to ‘accepted’.

Implemented in IIS 3.2.0.

**Related Release:**

Implemented in IIS 3.2.0.

**Status:** Implemented