NANC 360

**Doc Only Change Order for Recovery: Maximum TN Recovery Tunable**

**Origination Date :**04/12/2002

**Originator:**Neustar

**Description:**

A recent business situation has created an implementation of a new Service Provider-specific tunable.  This doc-only change order will add this definition to the appropriate documentation.

**Final Resolution:**

Func Backwards Compatible:  YES

Change the current documentation to explicitly state that the Service Provider-specific tunable (Maximum\_TN\_Recovery) is a tunable with a range of 1-10000, a default value of 2000, and is applicable for time-based recovery.

**Jan ’03 LNPAWG**, approved, move to next documentation category.

Implemented in FRS 3.2.1a and IIS 3.2.1a and GDMO 3.3.0.

**Related Release:**

Implemented in FRS 3.2.1a and IIS 3.2.1a and GDMO 3.3.0.

**Status:** Implemented