NANC 364

**Doc Only Change Order for ASN.1: Create Action comment**

**Origination Date :**07/15/2002

**Originator:**Neustar

**Description:**

A comment should be removed.  According to the current specification, the TN Range attribute is related to Release 1.4 pooling.  However, optional attribute is valid for other downloads to the LSMS.  This change order requests that the comment be removed to avoid confusion.

Below is an excerpt of the ASN.1 definition for the CreateAction:

LocalSMS-CreateAction ::= SEQUENCE {

   actionId INTEGER,

   subscriptionVersionObjects SET OF SubscriptionVersionObject,

   tn-range TN-Range OPTIONAL -- used only on pooled ports for release 1.4

}

**Final Resolution:**

Pure Backwards Compatible:  YES

Change the current documentation by removing the “used only on pooled ports for release 1.4”.

**Jan ’03 LNPAWG**, approved, move to next documentation category.

Implemented in ASN.1 3.3.0.

**Related Release:**

Implemented in ASN.1 3.3.0.

**Status:** Implemented