NANC 383

**Separate SOA channel for notifications**

**Origination Date :**05/06/2003

**Originator:**LNPA WG Archcture Planning Team

**Description:**

**Business Need:**(somewhat related to the existing ILL 5 and NANC 353 change orders).

This change order will separate out notifications with other messages, such that a separate channel will be established for SOA notifications versus all other SOA messages.  This performance related change order allows additional throughput on both channels.

**Final Resolution:**

Func Backwards Compatible:  YES

In order to separate out SOA notifications from all other SOA messages, additional processing logic will need to be developed.

Implemented in FRS 3.3.0a, GDMO 3.3.0 and ASN.1 3.3.0.

**Related Release:**

Implemented in FRS 3.3.0a, GDMO 3.3.0 and ASN.1 3.3.0.

**Status:** Implemented