Update Appendix E Download File Examples, Notifications Download File to reflect the SV Type and Alternative SPID attributes in the numberPoolBlock-objectCreation and numberPoolBlock-attributeValueChange notifications:

In the numberPoolBlock-objectCreation notification add the following rows:

|  |  |  |
| --- | --- | --- |
| 23 | SV Type | ( 0 )  Not present if the service provider does not support the SV Type.  If the service provider supports SV Type the value would be as defined in the Number Pooling Block Holder Information Data Model. |
|  24 | Alternative SPID | ( 2020 ) Not present if the service provider does not support the Alternative SPID.  If the service provider supports Alternative SPID but this attribute is not part of the number pool block, the pipes would be empty, otherwise if it were present the value would be as defined in the Number Pooling Block Holder Information Data Model. |

In the numberPoolBlock-attributeValueChange notification add the following rows:

|  |  |  |
| --- | --- | --- |
| 20 | SV Type | ( 0 )  Not present if the service provider does not support the SV Type.  If the service provider supports SV Type the value would be as defined in the Number Pooling Block Holder Information Data Model. |
|  21 | Alternative SPID | ( 2020 ) Not present if the service provider does not support the Alternative SPID.  If the service provider supports Alternative SPID but this attribute is not part of the number pool block, the pipes would be empty, otherwise if it were present the value would be as defined in the Number Pooling Block Holder Information Data Model. |