NANC 426

**Provide Modify Request Data to the SOA from Mass Updates**

**Origination Date :**10/10/2007

**Originator:**VeriSign

**Description:**

**Business Need:**

 (PIM 66) – Currently, when the NPAC conducts a mass update (modify-active) for a SOA customer; the SOA does not receive any notifications containing the modified attributes.  For SOAs that maintain SV data beyond the time of port activation, this creates an out-of-synch situation between the SOA database and the NPAC database.

**Final Resolution:**

Backward Compatible:  YES

The NPAC SMS would add a tunable parameter to the SPID-level customer profile that could be set to allow the sending/suppression of modify data to the respective SOA as a result of a mass update (modify-active).

Implemented in FRS 3.4.0a 3/19/10

 Implemented in IIS 3.4.0a 3/191/10

**Related Release:**

Implemented in FRS 3.4.0a 3/19/10

 Implemented in IIS 3.4.0a 3/191/10

**Status:** Implemented