**Origination Date:** 09/03/15

**Originator:** iconectiv

### Change Order Number: NANC 467

**Description:** ASN.1 – CMIP lnpRecoveryComplete Action reply

**Functional Backwards Compatible:** Yes

**IMPACT/CHANGE ASSESSMENT**

|  |  |  |
| --- | --- | --- |
| DOC | FRS | IIS |
| N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CMIP | GDMO | ASN.1 | **NPAC** | SOA | LSMS |
| N | Y | N | N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| XML | XIS | XSD | **NPAC** | SOA | LSMS |
| N | N | N | N | N |

**Business Need**

Recovery - CMIP lnpRecoveryComplete Action reply - RecoveryCompleteReply definition in ASN.1 contains subscriber-data, network-data, block-data. However, all of the subscription, network and block data is recovered via other messages, not the recovery complete message. These attributes seem to be unnecessary, and if so, can they be removed from ASN.1?

**Description of Change:**

Delete attributes.

ASN.1:

RecoveryCompleteReply ::= SEQUENCE {

status ResultsStatus,

~~subscriber-data [1] SubscriptionDownloadData OPTIONAL,~~

~~network-data [2] NetworkDownloadData OPTIONAL,~~

~~block-data [3] BlockDownloadData OPTIONAL,~~

error-code [~~4~~1] LnpSpecificErrorCode OPTIONAL -- present if status not success

}