**Origination Date:** 09/03/15

**Originator:** iconectiv

**Change Order Number: NANC 474 Description:** ASN.1 – SWIM Recovery

# Functional Backwards Compatible: Yes

**IMPACT/CHANGE ASSESSMENT**

DOC FRS IIS N N

CMIP GDMO ASN.1

# NPAC

SOA LSMS

N Y N N N

XML XIS XSD

# NPAC

SOA LSMS

N N N N N

# Business Need

Is the additionalInformation field in the M-EVENT-REPORT Reply SwimProcessing-RecoveryResponse ever populated?

# Description of Change:

Remove the additionlInformation attribute from the ASN.1. ASN.1:

SwimProcessing-RecoveryResponse ::= SEQUENCE { status [0] SwimResultsStatus,

error-code [1] LnpSpecificErrorCode OPTIONAL, -- present if status not success

stop-date [2] GeneralizedTime OPTIONAL, -- present if SWIM data collection turned off

~~additionalInformation [3] AdditionalInformation OPTIONAL~~

}