**Origination Date:** 08/12/16

**Originator:** iconectiv

### Change Order Number: NANC 487

**Description:** IIS/EFD Doc-Only Clarifications

**Functional Backwards Compatible:** Yes

**IMPACT/CHANGE ASSESSMENT**

|  |  |  |
| --- | --- | --- |
| DOC | FRS | IIS |
| N | Y |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CMIP | GDMO | ASN.1 | **NPAC** | SOA | LSMS |
| N | N | N | N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| XML | XIS | XSD | **NPAC** | SOA | LSMS |
| N | N | N | N | N |

**Business Need**

Documentation updates.

**Description of Change:**

Changes detailed below.

IIS:

NPAC SMS (changed text in yellow highlights)

EFD, Appendix A

Exhibit 3 CMIP Error Mapping to NPAC SMS Errors

| SMS Error | | Description | CMIP Error | | Description | |
| --- | --- | --- | --- | --- | --- | --- |
| [snip] |  | | |  | |  |
| 7235 | Query exceeds maximum tunable length. | | | ~~6~~10 | | ~~invalidAttributeValue~~ processingFailure\_er |
| [snip] |  | | |  | |  |