**Origination Date:** 02/14/18

**Originator:** iconectiv

### Change Order Number: NANC 518

**Description:** FRS Doc-only Clarifications

**Functional Backwards Compatible:** Yes

**IMPACT/CHANGE ASSESSMENT**

|  |  |  |
| --- | --- | --- |
| DOC | FRS | IIS |
| Y | N |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CMIP | GDMO | ASN.1 | **Neustar NPAC** | iconectiv NPAC | SOA | LSMS |
| N | N | N | N | N | N |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| XML | XIS | XSD | **Neustar NPAC** | iconectiv NPAC | SOA | LSMS |
| N | N | N | N | N | N |

**Business Need**

Documentation updates.

**Description of Change:**

Update the FRS requirements concerning creating a PTO SV to remove the PTO indicator from the validation (since the PTO indicator is required in any SV Create request). Two requirements need updating, one for inter-service provider ports and one for intra-service provider ports.

Requirements:

Section *5.1.2.2.1.1 - Subscription Version Creation - Inter-Service Provider Ports*

 [snip]

**RR5-179 Create Inter-Service Provider PTO Subscription Version - New Service Provider Data Attributes – Rejected**

NPAC SMS shall reject an Inter-Service Provider Create Request that includes the following data attributes from NPAC personnel or the new Service Provider, when the Porting to Original flag is set to True: (reference NANC 399).

• LRN

• Class DPC

• Class SSN

• LIDB DPC

• LIDB SSN

• CNAM DPC

• CNAM SSN

• ISVM DPC

• ISVM SSN

• WSMSC DPC (if supported by the Service Provider SOA)

• WSMSC SSN (if supported by the Service Provider SOA)

~~• Porting to Original~~

• Billing Service Provider ID

• End-User Location - Value

• End-User Location - Type

• SV Type

• Alternative SPID

[snip]

*Section 5.1.2.2.1.2 Subscription Version Creation - Intra-Service Provider Port*

[snip]

**RR5-180 Create “Intra-Service Provider Port” (PTO) Subscription Version – Current Service Provider Data Attributes – Rejected**

NPAC SMS shall reject an Intra-Service Provider Create Request that includes the following data attributes from NPAC personnel or the Current Service Provider, when the Porting to Original flag is set to True: (reference NANC 399)

* LRN
* Class DPC
* Class SSN
* LIDB DPC
* LIDB SSN
* CNAM DPC
* CNAM SSN
* ISVM DPC
* ISVM SSN
* WSMSC DPC (if supported by the Service Provider SOA)
* WSMSC SSN (if supported by the Service Provider SOA)
* ~~Porting to Original~~
* Billing Service Provider ID
* End-User Location - Value
* End-User Location – Type
* SV Type
* Alternative SPID

[snip]