**Origination Date:** 09/07/2019

**Originator:** iconectiv

### Change Order Number: NANC 544

**Description:** FRS – Doc-only Changes

**Functional Backwards Compatible:** Yes

**IMPACT/CHANGE ASSESSMENT**

|  |  |  |
| --- | --- | --- |
| DOC | FRS | IIS |
| Y | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CMIP | GDMO | ASN.1 | **NPAC** | SOA | LSMS |
| N | N | N | N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| XML | XIS | XSD | **NPAC** | SOA | LSMS |
| N | N | N | N | N |

**Business Need**

Documentation update.

**Description of Change:**

Changes detailed below.

FRS:

1. Add MMS to the Glossary:

MMS – MultiMedia Messaging Service; an MMS URI can be identified on subscription versions and number pool blocks.
2. The Data Integrity Audit in NANC 461 was sunset and although all requirements associated with the Data Integrity Audit have been deleted in previous versions of the FRS, there are 2 tunable parameters in Appendix C that need to be removed:

|  |  |  |  |
| --- | --- | --- | --- |
| **~~Data Integrity Sample Size~~**  | ~~1000~~ | ~~SVs~~ | ~~1-5000~~ |
| ~~The number of active Subscription Versions in a sample to be monitored by the NPAC SMS.~~  |
| **~~Data Integrity Sample Frequency~~**  | ~~7~~ | ~~Days~~ | ~~1-90~~ |
| ~~The interval in days between Data Integrity Samples conducted by the NPAC SMS.~~  |

1. Change the NPAC website reference in the Section 2 introduction paragraph, Section 2.1.2, 2.1.4, Appendix A (Process Flows) and Appendix E SV, Block, and Notification BDD file definitions to the iconectiv website name:

www.numberportability.com